**190-6682 - BREAKER, HYD,75FT/LB, 1T & MICRO**

**Bobcat**

**HB280**

|  |  |
| --- | --- |
| Operating Weight | 127 lb |
| Length | 34.1 in |
| Width | 7.9 in |
| Height | 9.8 in |
| Blows per minute | 1290 |
| Blows per minute Flow | 6 gal/min |
| Impact Energy Class | 60 ft-lb. (81 J) |
| Tool Diameter | 1.5 in |