Cylinder Storage Cage

Model RV-43-12C

 

Application:

* Storage of cylinders on industrial or construction sites
* Ideal for maximum of 6 x 100lb propane cylinders or 12 typical
* oxygen & acetylene size cylinders

Specifications:

* Length = 37”
* Width = 49”
* Height = 74”
* Weight empty = 345lbs

Features:

* Allows sites to remain compliant with regulated storage needs
* Able to padlock to prevent tampering
* Vented to prevent accumulation of fuel should a cylinder leak
* Roof to prevent accumulation of snow